Crank  RH  

09262-40008

Crank LH

09262-45011

Trans 

BEARING, RH (20X42X12)
09262-20059  20106????

Counter shaft

BEARING, LH (25X62X17)
09262-25083 09262-25125   25066?

Intermediate

BEARING, RH (22X56X16)   
09262-22028     22025??

BEARING, LH (17X40X12)    ?????  09262-17023 

09262-17046 

I already deglazed the cylinder. Got a nice cross hatch. Called me, they said the ring gaps should be at .016 and no less. They also said either 180 or 120 degrees is fine as they will walk a little anyways.